|  |  |  |
| --- | --- | --- |
| **Key Features** | | |
|  |  | Optimized unrestricted flow  Efficient on most sediments including rocks  Compact design and standardized components  Light weighted and very durable materials  Easy to install and ROV friendly  Backflush Hydraulic System  Low Pressure Water jetting system with separate nozzle |

|  |  |  |  |
| --- | --- | --- | --- |
| **Specifications** | |  | |
| Approx. weight in air |  | 110kg | |
| Approx. weight in water |  | 90kg | |
| Max hydraulic Flow |  | 70 lpm | |
| Max hydraulic Pressure |  | 200 bar | |
| Flow rate and removal capacity (theoretical) |  | Water flow at pump:  Gross water flow:  Removal capacity sand:  Removal capacity rocks:  Max rock size: | 1400 lpm  8108 lpm  84 T/hr  41 T/hr  140mm |
| Hydraulic Interface |  | Pressure:  Return:  Drain:  Backflush Close:  Backflush Open: | ¾ Hose / JIC 12  ¾ Hose / JIC 12  ½ Hose / JIC 8  ¼ Hose / JIC 4  ¼ Hose / JIC 4 |